**Highlights**

* Significant modifications in the structural and junction parameters of ZnSe/n-Si heterojunction is noticed after gamma irradiation.
* A direct dependence of barrier height (ΦB) on the lattice mismatch of ZnSe/n-Si heterojunction is noticed for different irradiation doses.